2026 May 17
++++++++++++++++++++++++++++
Changes to x32 Firmware Pack
++++++++++++++++++++++++++++
		FAI Requirement:
 1.-	Altimeter will give 900 microseconds pulse signal any time the input throttle signal is below OFF value (1200 microsecs)
 2.-	Altimeter will not give signal above OFF value until a input signal below OFF value (1200microseconds) has been validated.
 
NOTE: For compatibility these two requiremments are now ported to all of our Fw´s x.32

*******************************************************************************************************************************
****** WARNING: This change may need recalibration of your ESC and/or reconfiguration of your Throttle mixes in your transmitter
****** SAFETY FIRST: Carefully check results of this Fw change in your model´s behaviour
****** We recommend to do a trial test in ground in free space or with propeller removed
********************************************************************************************************************************

 3.- UI must be updated to align Throttle_in and Throttle_out signals in plots
 4.- UI now compatible with F3G records in plots, It now shows Motor time by default
 5.- UI only lets the user change values of those setting that the Fw´s formula allow (i.e. change things only in STD Fw)
 6.- Improved altitude records in initial seconds (it showed sometimes field elevation)
 7.- Stability improvement for PICO in AP mode: less oveheating 
	(We still recommend heat dissipation and/or reduce voltage to 5.0. volts for AP Mode)
 8.- More easy to open session (an indication appears in the message, Android users)
 9.- STA mode Allows for a Wi-Fi password of 8 characters (largely desired...)
10.- Reset via Magnetic reset switch in only F3G and F5L 
11.- "Weird PICO display" bug eliminated, only a few cases.
12.- Better behaviour for GliderKeeper App


